i emergency stop
i cut is down
i cut is up
i press is down
i press is up
i press in service
i manual back
i manual fwd
i drop done
i drop home
i push up
i push down
i push turn home
i push side
i push front
i push home
i push+pos
i hydr.preasure low
i hydr.temp high
i hydr.level low
i light port
i reserved
i keep up
i bending up
i bending mid
i bending down
i lower blade down
i lower blade up
i pos.slow
i pos.stop
i pos.over
i punch down
i punch up
i man conv
i hydr.filter
i creasing low 1
i creasing preasure 1
i creasing preasure 2
i haspel ready
i haspel auto
i foot pedal
i jack home
i jack down
i drop home
i drop done
i stacker home
i stacker up
i stacker turn
i stacker tilt
i stacker tilt home
i reverse limit
i wrapping machine
i sheet detect 1
i sheet detect 2
i felt system error
i felt min
i felt apply done
i felt cut done
i cap detector

o emergency stop
o cut down
o cut up
o press down
o press up
o lower bulk up
o hydr. on/off
o spray
o drop
o drop home
o ejector
o haspel
o push down
o push up
o push back
o push ret
o do push
o push turn
o hydr.start
o hydr.circ.
o preasure accum.reset
o light port reset
o reserved
o keep down
o bending down
o bending up
o lower blade up
o punch down
o central greesing
o creasing 1
o creasing 2
o free flow
o jack up
o jack down
o stacker
o stacker up
o stacker down
o stacker tilt
o stacker turn
o lightp. pass
o side lift down
o side lift up
o side lift
o conveyer
o ejector 1
o ejector 2
o line 2
o punch2 down
o felt apply
o felt cut

